|  |  |  |
| --- | --- | --- |
| **d9002 logo CMC** | **SOFTWARE RELEASE** | Compressor & Machine Controls N.V.  Industriepark Klein Frankrijk 62/05  B-9600 Ronse  Belgium |

# Release information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Release reference** | **Product Name** | **Module Name** | **Soft Name** | **Version #** |
| **F6205** | **SCADAR** | **SCADAR** | **{SY1217.00** | **16.0.0.0** |

# Approvals

|  |  |  |
| --- | --- | --- |
| **Responsibilities** | **Name** | **Date** |
| Prepared by engineering | Thibaut Stevens | 23/02/2018 |
| Reviewer | Thibaut Stevens | 23/02/2018 |
| Engineering peer approval | / | / |
| Product management | Graham Coats | 23/02/2018 |
| Customer approval (if required) |  |  |
| Pre production test |  |  |
| Quality approval |  |  |
| Production release implementation |  |  |

# Contents of this Release

## New feature Implemented

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Eng  by | Val  by | Ref |
| 8783 | CT: creating compressor table with CAGI tables | American and Canadian users can now optionally use the CAGI compressor table input popup. | **TS** | **TS** | **1** |
| 6519 | Compressor table bulk upload. | Admins can now bulk upload compressor tables. | **TS** | **TS** |  |
| 8746 | Clear unused / incorrect brand names | Clean up the list of brand names. | **TS** | **TS** |  |
|  |  |  |  |  |  |

## Bugs Fixed:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Eng  by | Val  by | Ref |
| 5775 | GW: difficulty opening graph styles | Graph styles crash on opening. | **TS** | **TS** |  |
| 2135 | AW : Piston compressor table, offload power not permitting 0 | Piston compressors are now allowed 0 kW offload. | **TS** | **TS** |  |
| 5708 | “Save as” function of compressor table is not functioning correctly | Bug in the saving of the model in compressor table “save as” functionality. | **TS** | **TS** |  |
| 5773 | GW: flow logged data axis is out of frame. | Switched the logged data axis of the flow logger to the left side of the graph. | **TS** | **TS** |  |
| 5774 | AW: wrong supply voltage in the “edit installation conditions” section | When adding an existing compressor table to a cs logger configuration, the wrong supply voltage is shown in the "Edit installation conditions" section. | **TS** | **TS** |  |
| 5762 | LP: Change AirInsite support link. | Change both landingspage tiles to http://support.air-insite.com/support/solutions/folders/33000201175 for the AirInsite skins. | **TS** | **TS** |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |