|  |  |  |
| --- | --- | --- |
| **d9002 logo CMC** | **SOFTWARE RELEASE** | Compressor & Machine Controls N.V.Industriepark Klein Frankrijk 62/05B-9600 RonseBelgium |

# Release information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Release reference** | **Product Name** | **Module Name** | **Soft Name** | **Version #** |
| **F6205** | **SCADAR** |  | **{SY1217.00** | **16.1.0.0** |

# Approvals

|  |  |  |
| --- | --- | --- |
| **Responsibilities** | **Name** | **Date** |
| Prepared by engineering | Thibaut Stevens  | 18/06/2018 |
| Reviewer | Pieter Eggermont | 18/06/2018 |
| Engineering peer approval | Pieter Eggermont | 18/06/2018 |
| Product management | Graham Coats | 18/06/2018 |
| Customer approval (if required) |  |  |
| Pre production test |  |  |
| Quality approval |  |  |
| Production release implementation |  |  |

# Contents of this Release

## New feature Implemented

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 9033 | UA : expand user list export | Expanded the columns of the export user list. | **TS** | **TS** | **1** |
| 9007 | Unlimited sync quota | Added the options for Auditors to add an unlimited sync quota to the consultant subscription. | **TS** | **TS** |  |
| 8786 | Limit admin access to other admin accounts and system | Limited the admin access and added a product manager role. | **TS** | **TS** |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

## Bugs Fixed:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 5790 | UA: data shifted 2 seconds in data export | Start time shift when creating the data export | **TS** | **TS** |  |
| 5789 | PW: footer does not update correctly | Footer changes are now propagated to other footer elements | **TS** | **TS** |  |
| 5788 | PW: audit duplicates on landings page | Shared audit appeared twice in audit lists. | **TS** | **TS** |  |
| 5786 | PW: missing logo’s in report |  | **TS** | **TS** |  |
| 5783 | GW: GP loggers not used in system flow | GP stream needed to be converted from 4-20mA to flow values before being used. | **TS** | **TS** |  |
| 5782 | SW: can’t open audit-less simulation collection | Needed to perform an extra check on the availability of audit start and end time. | **TS** | **TS** |  |
| 5781 | SW: investigate kWh inconsistency | Made rounding issue less noticeable. | **TS** | **TS** |  |
| 5780  | Data export: system power calculations | Use calculated datastreams where needed iso measured ones. | **TS** | **TS** |  |
|  |  |  |  |  |  |

# Verification

|  |  |
| --- | --- |
| **Ref** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |