|  |  |  |
| --- | --- | --- |
| **d9002 logo CMC** | **SOFTWARE RELEASE** | Compressor & Machine Controls N.V.Industriepark Klein Frankrijk 62/05B-9600 RonseBelgium |

# Release information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Release reference** | **Product Name** | **Module Name** | **Soft Name** | **Version #** |
| **F6205** | **SCADAR** | **SCADAR** | **{SY1217.00** | **15.10.0.0** |

# Approvals

|  |  |  |
| --- | --- | --- |
| **Responsibilities** | **Name** | **Date** |
| Prepared by engineering | Thibaut Stevens  | 15/12/2017 |
| Reviewer | Thibaut Stevens | 15/12/2017 |
| Engineering peer approval | / | / |
| Product management | Graham Coats | 15/12/2017 |
| Customer approval (if required) |  |  |
| Pre production test |  |  |
| Quality approval |  |  |
| Production release implementation |  |  |

# Contents of this Release

## New feature Implemented

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 8930 | AM: Daily or single data export worksheet | Users get the option of creating a data export file with a single worksheet or with a worksheet for each day. | **TS** | **TS** | **1** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

## Bugs Fixed:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 5740 | AW: audit duplicates in landingspages. | An audit will appear multiple times in the landingspage audit list. Once for each time it has been shared with a user. | **TS** | **TS** |  |
| 5741 | AM: kW not shown in the data export | The measured kW’s were always shown in the data export, even when the “calculate my kW” checkmark was on. | **TS** | **TS** |  |
| 5742 | AW: flow meter pipe resizing not updated | Asynchronous timing issue caused the flow logger’s min and max update to fail when pressing OK directly after changing the diameter. | **TS** | **TS** |  |
| 5742 | AM: formatting in data export excel | Format the numbers as numbers and not as text, while keeping the number of spaces after the decimal separator. | **TS** | **TS** |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |