|  |  |  |
| --- | --- | --- |
| **d9002 logo CMC** | **SOFTWARE RELEASE** | Compressor & Machine Controls N.V.Industriepark Klein Frankrijk 62/05B-9600 RonseBelgium |

# Release information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Release reference** | **Product Name** | **Module Name** | **Soft Name** | **Version #** |
| **F6205** | **SCADAR** | **SCADAR** | **{SY1217.00** | **15.11.0.0** |

# Approvals

|  |  |  |
| --- | --- | --- |
| **Responsibilities** | **Name** | **Date** |
| Prepared by engineering | Thibaut Stevens  | 26/01/2018 |
| Reviewer | Thibaut Stevens | 26/01/2018 |
| Engineering peer approval | / | / |
| Product management | Graham Coats | 26/01/2018 |
| Customer approval (if required) |  |  |
| Pre production test |  |  |
| Quality approval |  |  |
| Production release implementation |  |  |

# Contents of this Release

## New feature Implemented

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 8951 | Dewpoint sensor calculate atmospheric dewpoint datastream | Dewpoint sensor logs at pressure and not at atmosphere. So we need to change the graphs and corresponding calculations. | **TS** | **TS** | **1** |
| 8952 | GW: add the 4-20mA data stream for the flow logger. | Show the 4-20mA in the flow logger graph in graph wizard. | **TS** | **TS** |  |
| 8953 | CW: general chart improvements | Made cosmetic improvements to chart wizard. | **TS** | **TS** |  |
| 8954 | GW: solid line for system demand flow when measured | System demand side is a solid line when the back end returns the system measured flow to the front end. | **TS** | **TS** |  |
| 8965 | LP: draw more attention to the software version number. | A blinking lightbulb will be shown next to the version number until a week has passed since last release or the user has clicked on the link. | **TS** | **TS** |  |
| 8966 | GW: improve tooltip | Add the text ‘DISPLAY MODE: ‘ before the actual display mode. | **TS**  | **TS** |  |
|  |  |  |  |  |  |

## Bugs Fixed:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ontime ID | Name | Description | Engby | Valby | Ref |
| 5759 | AW: Auditlist ignored unfinished audits | Auditlist ignores audits that haven't reached step 4 in audit wizard. | **TS** | **TS** |  |
| 5756 | GW: flow measurements incorrect | Wrong conversion when adjusting the diameter in audit wizard step 2. | **TS** | **TS** |  |
| 5755 | SW: Audit-less simulation fails | Adding a compressor to the red line results in crash. | **TS** | **TS** |  |
| 5754 | AM: File name invalid character filter | The data export file name filter for invalid characters is incomplete. Audit names with / or : are not filtered out | **TS** | **TS** |  |
| 5753 | AM: DS wrong number format | Data stream for the dewpoint sensor logged data had the wrong number format in the data export file. | **TS** | **TS** |  |
| 5752 | LP: Users don’t see the software version. | Users can't see the scadar software version number on the landingspage. | **TS** | **TS** |  |
| 5751 | GW: Users can’t update the compressor type. | PE already fixed the bug of updating crashing. This ticket is for actually updating the compressor table with the correct type. | **TS** | **TS** |  |
| 5748 | GW: previous and next zoom | Graph wizard zoom options previous and next are disabled because the zoom history is resetted each time we zoom and need to recollect the datastreams. | **TS** | **TS** |  |
| 5747 | GW: zoom reset button | Layover is not removed after done with resetting the graphs. | **TS** | **TS** |  |
| 5746 | GW: PF datastream hidden | User can't see the PF of one of his compressor. | **TS** | **TS** |  |
| 5758 | AW: BS error code only if valid SN. | Warning message is only shown when a user has entered a valid BaseStation SN. | **TS** | **TS** |  |
| 5761 | AM: Audit export data missing | Data export for flow and power have lines that didn’t have any data values. | **TS**  | **TS** |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |